**Job/Task:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EYES/FACE | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  airborne dust  flying particles  hazardous liquids/chemicals  intense light  blood splashes  other: | | PPE required to manage hazard:  safety glasses  safety goggles  face shield  shading/filter (#     )  welding shield  other: | | Comments: |
| HEAD | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  beams  pipes  falling objects  exposed electrical wiring or components  machine parts  other: | | PPE required to manage hazard:  protective helmet  Type A (low voltage)  Type B (high voltage)  Type C  hair net or soft cap  other: | | Comments: |
| HANDS/ARMS | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  hazardous liquids/chemicals  scrapes, bruises, or cuts  injuries from tools  extreme heat/cold  blood (OPIM)  other: | | PPE required to manage hazard:  gloves  chemical resistance  liquid/leak resistance  temperature resistance  cut resistance  gauntlet or long necked  work gloves  chemical protective sleeves  long sleeves  other: . | | Comments: |
| FEET/LEGS | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  hazardous liquids/chemicals  heavy falling/rolling objects  heavy equipment  exposed electrical wiring or components  slippery surfaces  explosive atmospheres  tools  other: | | PPE required to manage hazard:  closed shoes (e.g. no opened toes or sandals)  long pants  safety shoes or boots  toe protection  metatarsal protection  electrical protection  heat/cold protection  anti-slip soles  chemical resistance  leggings or chaps  foot-leg guards  other: | | Comments: |
| BODY/SKIN | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  hazardous liquids/chemicals  sharp or rough edges  extreme heat/cold  flash fire  other: | | PPE required to manage hazard:  lab coat  raingear  coveralls, body suit  apron  welding leathers  FRC clothing  abrasion/cut resistance  other: | | Comments: |
| BODY/WHOLE | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  working from heights of 10 feet or more  working near water  other: | | PPE required to manage hazard:  fall arrest/restraint: Type:  personal floatation device: Type:  other: | | Comments: |
| LUNGS/EARS | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  irritating dust or particulate  irritating or toxic gas/vapor  loud work environment  noisy machines/tools  other: | | PPE required to manage hazard:  respirator (cartridge type:      )  SCBA  SAR  particulate mask  hearing protection (minimum NRR:      ) | | Comments: |

**Job/Task:**

|  |
| --- |
| **Notes** |
|  |

|  |  |  |
| --- | --- | --- |
| **Revision/Review Log** | | |
| **Revision/Review Date** | **Revisions Made (or “Review Only”** | **Certification** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |