**Job/Task:**

|  |  |  |
| --- | --- | --- |
| EYES/FACE |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  airborne dust[ ]  flying particles[ ]  hazardous liquids/chemicals[ ]  intense light[ ]  blood splashes[ ]  other:       | PPE required to manage hazard:[ ]  safety glasses [ ]  safety goggles[ ]  face shield [ ]  shading/filter (#     ) [ ]  welding shield[ ]  other:       | Comments:      |
| HEAD |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  beams[ ]  pipes[ ]  falling objects[ ]  exposed electrical wiring or components[ ]  machine parts [ ]  other:       | PPE required to manage hazard:[ ]  protective helmet[ ]  Type A (low voltage)[ ]  Type B (high voltage)[ ]  Type C[ ]  hair net or soft cap[ ]  other:       | Comments:      |
| HANDS/ARMS |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  hazardous liquids/chemicals[ ]  scrapes, bruises, or cuts [ ]  injuries from tools [ ]  extreme heat/cold[ ]  blood (OPIM)[ ]  other:       | PPE required to manage hazard:[ ]  gloves[ ]  chemical resistance [ ]  liquid/leak resistance[ ]  temperature resistance [ ]  cut resistance[ ]  gauntlet or long necked [ ]  work gloves[ ]  chemical protective sleeves[ ]  long sleeves[ ]  other: . | Comments:      |
| FEET/LEGS |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  hazardous liquids/chemicals[ ]  heavy falling/rolling objects[ ]  heavy equipment [ ]  exposed electrical wiring or components[ ]  slippery surfaces[ ]  explosive atmospheres[ ]  tools[ ]  other:       | PPE required to manage hazard:[ ]  closed shoes (e.g. no opened toes or sandals)[ ]  long pants[ ]  safety shoes or boots[ ]  toe protection [ ]  metatarsal protection[ ]  electrical protection [ ]  heat/cold protection[ ]  anti-slip soles [ ]  chemical resistance[ ]  leggings or chaps [ ]  foot-leg guards[ ]  other:       | Comments:      |
| BODY/SKIN | [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  hazardous liquids/chemicals[ ]  sharp or rough edges [ ]  extreme heat/cold[ ]  flash fire[ ]  other:       | PPE required to manage hazard:[ ]  lab coat [ ]  raingear[ ]  coveralls, body suit [ ]  apron[ ]  welding leathers [ ]  FRC clothing [ ]  abrasion/cut resistance[ ]  other:  | Comments:      |
| BODY/WHOLE |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  working from heights of 10 feet or more[ ]  working near water[ ]  other:       | PPE required to manage hazard:[ ]  fall arrest/restraint: Type:      [ ]  personal floatation device: Type:      [ ]  other:       | Comments:      |
| LUNGS/EARS |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No [ ]**  |
| Work-related exposure to:[ ]  irritating dust or particulate[ ]  irritating or toxic gas/vapor[ ]  loud work environment[ ]  noisy machines/tools[ ]  other:       | PPE required to manage hazard:[ ]  respirator (cartridge type:      )[ ]  SCBA[ ]  SAR[ ]  particulate mask[ ]  hearing protection (minimum NRR:      )  | Comments:      |

**Job/Task:**

|  |
| --- |
| **Notes** |
|       |

|  |
| --- |
| **Revision/Review Log** |
| **Revision/Review Date** | **Revisions Made (or “Review Only”** | **Certification** |
|       |       |       |
|       |       |       |
|       |       |       |
|       |       |       |